,Colour##Other##,Description##Other##,Features##Other##,Finish##Other##,ModelFinish##Other##,ManufacturerURL##Other##,ModelNumber##Other##,Name##Other##,NominalHeight##LENGTH##MILLIMETERS,NominalLength##LENGTH##MILLIMETERS,NominalWidth##LENGTH##MILLIMETERS,ProductInformation##Other##,Size##Other##,TotalWattage##Other##,Wattage##ELECTRICAL_WATTAGE##WATTS,BIMObjectName##Other##,PhotometricFileName##Other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,LightSource##Other##,CTL##Other##,CTR##Other##
LED50-GEN2-22Degrees-2700K-80-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-27-22,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-22Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-624Lumen-22Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-22-500mA.ies,2700,1,0,1
LED50-GEN2-36Degrees-2700K-80-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-27-36,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-36Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-576Lumen-36Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-36-500mA.ies,2700,1,0,1
LED50-GEN2-36Degrees-3000K-80-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-30-36,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-36Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-658Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-36-500mA.ies,3000,1,0,1
LED50-GEN2-18Degrees-3000K-80-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-30-18,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-18Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-683Lumen-18Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-18-500mA.ies,3000,1,0,1
LED50-GEN2-22Degrees-3000K-80-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-30-22,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-22Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-715Lumen-22Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-22-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-18Degrees-3000K-90-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-30-18-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-18Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-869Lumen-18Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-18-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-36Degrees-3000K-90-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-30-36-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-36Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-823Lumen-36Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-36-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-22Degrees-3000K-90-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-30-22-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-22Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-883Lumen-22Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-22-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-36Degrees-2700K-90-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-27-36-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-36Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-813Lumen-36Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-36-90-500mA.ies,2700,1,0,1
LED50-GEN2-Plus-22Degrees-2700K-90-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50/2-27-22-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-22Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-867Lumen-22Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-22-90-500mA.ies,2700,1,0,1
LED50-Warm-Dim-36Degrees-3000K-80-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 Ambiance WarmDim Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED50WD-30-36,Pinhole_Edge_Accent_Trim_IP54-LED50_Warm_Dim-36Degrees-3000K-80-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,96 x 92 x 92,14.5,14.5,Xtech_Lucent_Pinhole_Edge-LED50_Warm_Dim-568Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED - LED50WD-30-36-700mA.ies,3000,2,0,1
LED50-One-GEN2-24Degrees-3000K-90-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 ONE GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED51/2-30-24,Pinhole_Edge_Accent_Trim_IP54-LED50_One_GEN2-24Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-LED50_One_GEN2-1082Lumen-24Degrees-3000K-90-CRI,91413-A_F-LED - LED51_2-30-24-350mA.ies,3000,2,0,1
LED50-One-Superspot-7Degrees-3000K-90-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with LED50 ONE SuperSpot Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PB-LED51-30-7,Pinhole_Edge_Accent_Trim_IP54-LED50_One_Superspot-7Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,6.7,6.7,Xtech_Lucent_Pinhole_Edge-LED50_One_Superspot-486Lumen-7Degrees-3000K-90-CRI,91413-A_F-LED - LED51SS-30-7-350mA.ies,3000,2,0,1
XTM-1300Lumen-55Degrees-3000K-83-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with Xicato XTM Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XTM-1300-30-55-5,Pinhole_Edge_Accent_Trim_IP54-XTM-55Degrees-3000K-83-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-XTM-1300Lumen-55Degrees-3000K-83-CRI,91413-XIC-XTM-0D-1300-xx-55-5-700.ies,3000,5,0,1
XTA-1300Lumen-55Degrees-2700K-98-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with Xicato XTA Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XTA-1300-27-55-5,Pinhole_Edge_Accent_Trim_IP54-XTA-55Degrees-2700K-98-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,15.6,15.6,Xtech_Lucent_Pinhole_Edge-XTA-1300Lumen-55Degrees-2700K-98-CRI,91413-XIC-XTA-0D-1300-xx-55-5-700.ies,2700,5,0,1
XTM9-1300Lumen-37Degrees-3000K-83-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with Xicato XTM9 Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XTM9-1300-30-37-5,Pinhole_Edge_Accent_Trim_IP54-XTM9-37Degrees-3000K-83-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,118 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XTM9-1300Lumen-37Degrees-3000K-83-CRI,91413-F_A-XIC - XTM09-0D-1300-xx-15-5-700mA.ies,3000,4,0,1
XTA9-37Degrees-3000K-98-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with Xicato XTA9 Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XTA9-700-30-37-5,Pinhole_Edge_Accent_Trim_IP54-XTA9-37Degrees-3000K-98-CRI-Lucent,85,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,85 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XTA9-37Degrees-3000K-98-CRI,91413-F_A-XIC - XTA09-0D-1300-xx-15-5-1050mA.ies,3000,3,0,1
XLED50-Shallow-Height-23Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XLED50-827-23-SH,Pinhole_Edge_Accent_Trim_IP54-XLED50_Shallow_Height-23Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-23Degrees-2700K-83-CRI,,2700,6,0,1
XLED50-Shallow-Height-35Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XLED50-827-35-SH,Pinhole_Edge_Accent_Trim_IP54-XLED50_Shallow_Height-35Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-35Degrees-2700K-83-CRI,,2700,6,0,1
XLED50-High-Efficency-35Degrees-3000K-83-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XLED50-830-35-HE,Pinhole_Edge_Accent_Trim_IP54-XLED50_High_Efficency-35Degrees-3000K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-35Degrees-3000K-83-CRI,,3000,7,0,1
XLED50-High-Efficency-23Degrees-2700K-83-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XLED50-827-23-HE,Pinhole_Edge_Accent_Trim_IP54-XLED50_High_Efficency-23Degrees-2700K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-23Degrees-2700K-83-CRI,,2700,7,0,1
XLED50-High-Output-23Degrees-2700K-83-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with XLED50 High Output Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XLED50-HO-927-23,Pinhole_Edge_Accent_Trim_IP54-XLED50_High_Output-23Degrees-2700K-83-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_Output-23Degrees-2700K-83-CRI,,2700,8,0,1
XLED50-Shallow-Height-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Shallow Height-Trim-White,RAL 9010,"Adjustable IP54 Pinhole Edge Trim with XLED50 Shallow Height, High CRI Module","Adjustable, IP54, Shallow Height",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XLED50-SH-90-930-23,Pinhole_Edge_Accent_Trim_IP54-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI,,3000,7,0,1
XLED50-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Trim-White,RAL 9010,Adjustable IP54 Pinhole Edge Trim with XLED50 High CRI Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PB-XLED50-90-930-23,Pinhole_Edge_Accent_Trim_IP54-XLED50_High_CRI-23Degrees-3000K-98-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_CRI-23Degrees-3000K-98-CRI,,3000,8,0,1
LED50-GEN2-22Degrees-2700K-80-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-27-22,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-22Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-624Lumen-22Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-22-500mA.ies,2700,1,1,0
LED50-GEN2-36Degrees-2700K-80-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-27-36,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-36Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-576Lumen-36Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-36-500mA.ies,2700,1,1,0
LED50-GEN2-36Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-30-36,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-36Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-658Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-36-500mA.ies,3000,1,1,0
LED50-GEN2-18Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-30-18,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-18Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-683Lumen-18Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-18-500mA.ies,3000,1,1,0
LED50-GEN2-22Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-30-22,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-22Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-715Lumen-22Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-22-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-18Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-30-18-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-18Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-869Lumen-18Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-18-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-36Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-30-36-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-36Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-823Lumen-36Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-36-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-22Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-30-22-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-22Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-883Lumen-22Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-22-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-36Degrees-2700K-90-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-27-36-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-36Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-813Lumen-36Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-36-90-500mA.ies,2700,1,1,0
LED50-GEN2-Plus-22Degrees-2700K-90-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50/2-27-22-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-22Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-867Lumen-22Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-22-90-500mA.ies,2700,1,1,0
LED50-Warm-Dim-36Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 Ambiance WarmDim Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED50WD-30-36,Pinhole_Edge_Accent_Trimless_IP54-LED50_Warm_Dim-36Degrees-3000K-80-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,96 x 92 x 92,14.5,14.5,Xtech_Lucent_Pinhole_Edge-LED50_Warm_Dim-568Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED - LED50WD-30-36-700mA.ies,3000,2,1,0
LED50-One-GEN2-24Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 ONE GEN2 Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED51/2-30-24,Pinhole_Edge_Accent_Trimless_IP54-LED50_One_GEN2-24Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-LED50_One_GEN2-1082Lumen-24Degrees-3000K-90-CRI,91413-A_F-LED - LED51_2-30-24-350mA.ies,3000,2,1,0
LED50-One-Superspot-7Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with LED50 ONE SuperSpot Module,Adjustable,Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-WH-PC-LED51-30-7,Pinhole_Edge_Accent_Trimless_IP54-LED50_One_Superspot-7Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,6.7,6.7,Xtech_Lucent_Pinhole_Edge-LED50_One_Superspot-486Lumen-7Degrees-3000K-90-CRI,91413-A_F-LED - LED51SS-30-7-350mA.ies,3000,2,1,0
XTM-1300Lumen-55Degrees-3000K-83-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with Xicato XTM Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XTM-1300-30-55-5,Pinhole_Edge_Accent_Trimless_IP54-XTM-55Degrees-3000K-83-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-XTM-1300Lumen-55Degrees-3000K-83-CRI,91413-XIC-XTM-0D-1300-xx-55-5-700.ies,3000,5,1,0
XTA-1300Lumen-55Degrees-2700K-98-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with Xicato XTA Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XTA-1300-27-55-5,Pinhole_Edge_Accent_Trimless_IP54-XTA-55Degrees-2700K-98-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,15.6,15.6,Xtech_Lucent_Pinhole_Edge-XTA-1300Lumen-55Degrees-2700K-98-CRI,91413-XIC-XTA-0D-1300-xx-55-5-700.ies,2700,5,1,0
XTM9-1300Lumen-37Degrees-3000K-83-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with Xicato XTM9 Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XTM9-1300-30-37-5,Pinhole_Edge_Accent_Trimless_IP54-XTM9-37Degrees-3000K-83-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,118 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XTM9-1300Lumen-37Degrees-3000K-83-CRI,91413-F_A-XIC - XTM09-0D-1300-xx-15-5-700mA.ies,3000,4,1,0
XTA9-37Degrees-3000K-98-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with Xicato XTA9 Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XTA9-700-30-37-5,Pinhole_Edge_Accent_Trimless_IP54-XTA9-37Degrees-3000K-98-CRI-Lucent,85,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,85 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XTA9-37Degrees-3000K-98-CRI,91413-F_A-XIC - XTA09-0D-1300-xx-15-5-1050mA.ies,3000,3,1,0
XLED50-Shallow-Height-23Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XLED50-827-23-SH,Pinhole_Edge_Accent_Trimless_IP54-XLED50_Shallow_Height-23Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-23Degrees-2700K-83-CRI,,2700,6,1,0
XLED50-Shallow-Height-35Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XLED50-827-35-SH,Pinhole_Edge_Accent_Trimless_IP54-XLED50_Shallow_Height-35Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-35Degrees-2700K-83-CRI,,2700,6,1,0
XLED50-High-Efficency-35Degrees-3000K-83-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XLED50-830-35-HE,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_Efficency-35Degrees-3000K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-35Degrees-3000K-83-CRI,,3000,7,1,0
XLED50-High-Efficency-23Degrees-2700K-83-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XLED50-827-23-HE,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_Efficency-23Degrees-2700K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-23Degrees-2700K-83-CRI,,2700,7,1,0
XLED50-High-Output-23Degrees-2700K-83-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with XLED50 High Output Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XLED50-HO-927-23,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_Output-23Degrees-2700K-83-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_Output-23Degrees-2700K-83-CRI,,2700,8,1,0
XLED50-Shallow-Height-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Shallow Height-Trimless-White,RAL 9010,"Adjustable IP54 Pinhole Edge Trimless with XLED50 Shallow Height, High CRI Module","Adjustable, IP54, Shallow Height",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XLED50-SH-90-930-23,Pinhole_Edge_Accent_Trimless_IP54-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI,,3000,7,1,0
XLED50-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Trimless-White,RAL 9010,Adjustable IP54 Pinhole Edge Trimless with XLED50 High CRI Module,"Adjustable, IP54",Powder Coat - Lucent - White RAL 9010,Xtech_Lucent_White_RAL9010,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-WH-PC-XLED50-90-930-23,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_CRI-23Degrees-3000K-98-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_CRI-23Degrees-3000K-98-CRI,,3000,8,1,0
LED50-GEN2-22Degrees-2700K-80-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-27-22,Pinhole_Edge_Accent_Trim-LED50_GEN2-22Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-624Lumen-22Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-22-500mA.ies,2700,1,0,1
LED50-GEN2-36Degrees-2700K-80-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-27-36,Pinhole_Edge_Accent_Trim-LED50_GEN2-36Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-576Lumen-36Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-36-500mA.ies,2700,1,0,1
LED50-GEN2-36Degrees-3000K-80-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-30-36,Pinhole_Edge_Accent_Trim-LED50_GEN2-36Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-658Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-36-500mA.ies,3000,1,0,1
LED50-GEN2-18Degrees-3000K-80-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-30-18,Pinhole_Edge_Accent_Trim-LED50_GEN2-18Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-683Lumen-18Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-18-500mA.ies,3000,1,0,1
LED50-GEN2-22Degrees-3000K-80-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-30-22,Pinhole_Edge_Accent_Trim-LED50_GEN2-22Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-715Lumen-22Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-22-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-18Degrees-3000K-90-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-30-18-90,Pinhole_Edge_Accent_Trim-LED50_GEN2_Plus-18Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-869Lumen-18Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-18-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-36Degrees-3000K-90-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-30-36-90,Pinhole_Edge_Accent_Trim-LED50_GEN2_Plus-36Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-823Lumen-36Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-36-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-22Degrees-3000K-90-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-30-22-90,Pinhole_Edge_Accent_Trim-LED50_GEN2_Plus-22Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-883Lumen-22Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-22-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-36Degrees-2700K-90-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-27-36-90,Pinhole_Edge_Accent_Trim-LED50_GEN2_Plus-36Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-813Lumen-36Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-36-90-500mA.ies,2700,1,0,1
LED50-GEN2-Plus-22Degrees-2700K-90-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50/2-27-22-90,Pinhole_Edge_Accent_Trim-LED50_GEN2_Plus-22Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-867Lumen-22Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-22-90-500mA.ies,2700,1,0,1
LED50-Warm-Dim-36Degrees-3000K-80-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 Ambiance WarmDim Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED50WD-30-36,Pinhole_Edge_Accent_Trim-LED50_Warm_Dim-36Degrees-3000K-80-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,96 x 92 x 92,14.5,14.5,Xtech_Lucent_Pinhole_Edge-LED50_Warm_Dim-568Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED - LED50WD-30-36-700mA.ies,3000,2,0,1
LED50-One-GEN2-24Degrees-3000K-90-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED51/2-30-24,Pinhole_Edge_Accent_Trim-LED50_One_GEN2-24Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-LED50_One_GEN2-1082Lumen-24Degrees-3000K-90-CRI,91413-A_F-LED - LED51_2-30-24-350mA.ies,3000,2,0,1
LED50-One-Superspot-7Degrees-3000K-90-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with LED50 ONE SuperSpot Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PB-LED51-30-7,Pinhole_Edge_Accent_Trim-LED50_One_Superspot-7Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,6.7,6.7,Xtech_Lucent_Pinhole_Edge-LED50_One_Superspot-486Lumen-7Degrees-3000K-90-CRI,91413-A_F-LED - LED51SS-30-7-350mA.ies,3000,2,0,1
XTM-1300Lumen-55Degrees-3000K-83-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with Xicato XTM Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XTM-1300-30-55-5,Pinhole_Edge_Accent_Trim-XTM-55Degrees-3000K-83-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,132 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-XTM-1300Lumen-55Degrees-3000K-83-CRI,91413-XIC-XTM-0D-1300-xx-55-5-700.ies,3000,5,0,1
XTA-1300Lumen-55Degrees-2700K-98-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with Xicato XTA Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XTA-1300-27-55-5,Pinhole_Edge_Accent_Trim-XTA-55Degrees-2700K-98-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,132 x 92 x 92,15.6,15.6,Xtech_Lucent_Pinhole_Edge-XTA-1300Lumen-55Degrees-2700K-98-CRI,91413-XIC-XTA-0D-1300-xx-55-5-700.ies,2700,5,0,1
XTM9-1300Lumen-37Degrees-3000K-83-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with Xicato XTM9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XTM9-1300-30-37-5,Pinhole_Edge_Accent_Trim-XTM9-37Degrees-3000K-83-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,118 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XTM9-1300Lumen-37Degrees-3000K-83-CRI,91413-F_A-XIC - XTM09-0D-1300-xx-15-5-700mA.ies,3000,4,0,1
XTA9-37Degrees-3000K-98-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with Xicato XTA9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XTA9-700-30-37-5,Pinhole_Edge_Accent_Trim-XTA9-37Degrees-3000K-98-CRI-Lucent,85,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,85 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XTA9-37Degrees-3000K-98-CRI,91413-F_A-XIC - XTA09-0D-1300-xx-15-5-1050mA.ies,3000,3,0,1
XLED50-Shallow-Height-23Degrees-2700K-83-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XLED50-827-23-SH,Pinhole_Edge_Accent_Trim-XLED50_Shallow_Height-23Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-23Degrees-2700K-83-CRI,,2700,6,0,1
XLED50-Shallow-Height-35Degrees-2700K-83-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XLED50-827-35-SH,Pinhole_Edge_Accent_Trim-XLED50_Shallow_Height-35Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-35Degrees-2700K-83-CRI,,2700,6,0,1
XLED50-High-Efficency-35Degrees-3000K-83-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XLED50-830-35-HE,Pinhole_Edge_Accent_Trim-XLED50_High_Efficency-35Degrees-3000K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-35Degrees-3000K-83-CRI,,3000,7,0,1
XLED50-High-Efficency-23Degrees-2700K-83-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XLED50-827-23-HE,Pinhole_Edge_Accent_Trim-XLED50_High_Efficency-23Degrees-2700K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-23Degrees-2700K-83-CRI,,2700,7,0,1
XLED50-High-Output-23Degrees-2700K-83-CRI-Adjustable-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with XLED50 High Output Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XLED50-HO-927-23,Pinhole_Edge_Accent_Trim-XLED50_High_Output-23Degrees-2700K-83-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_Output-23Degrees-2700K-83-CRI,,2700,8,0,1
XLED50-Shallow-Height-High-CRI-23Degrees-3000K-98-CRI-Adjustable-Trim-Black,RAL 9005,"Adjustable Pinhole Edge Trim with XLED50 Shallow Height, High CRI Module","Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XLED50-SH-90-930-23,Pinhole_Edge_Accent_Trim-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,96 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI,,3000,7,0,1
XLED50-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable Pinhole Edge Trim with XLED50 High CRI Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PB-XLED50-90-930-23,Pinhole_Edge_Accent_Trim-XLED50_High_CRI-23Degrees-3000K-98-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_CRI-23Degrees-3000K-98-CRI,,3000,8,0,1
LED50-GEN2-22Degrees-2700K-80-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-27-22,Pinhole_Edge_Accent_Trimless-LED50_GEN2-22Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-624Lumen-22Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-22-500mA.ies,2700,1,1,0
LED50-GEN2-36Degrees-2700K-80-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-27-36,Pinhole_Edge_Accent_Trimless-LED50_GEN2-36Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-576Lumen-36Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-36-500mA.ies,2700,1,1,0
LED50-GEN2-36Degrees-3000K-80-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-30-36,Pinhole_Edge_Accent_Trimless-LED50_GEN2-36Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-658Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-36-500mA.ies,3000,1,1,0
LED50-GEN2-18Degrees-3000K-80-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-30-18,Pinhole_Edge_Accent_Trimless-LED50_GEN2-18Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-683Lumen-18Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-18-500mA.ies,3000,1,1,0
LED50-GEN2-22Degrees-3000K-80-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-30-22,Pinhole_Edge_Accent_Trimless-LED50_GEN2-22Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-715Lumen-22Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-22-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-18Degrees-3000K-90-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-30-18-90,Pinhole_Edge_Accent_Trimless-LED50_GEN2_Plus-18Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-869Lumen-18Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-18-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-36Degrees-3000K-90-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-30-36-90,Pinhole_Edge_Accent_Trimless-LED50_GEN2_Plus-36Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-823Lumen-36Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-36-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-22Degrees-3000K-90-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-30-22-90,Pinhole_Edge_Accent_Trimless-LED50_GEN2_Plus-22Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-883Lumen-22Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-22-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-36Degrees-2700K-90-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-27-36-90,Pinhole_Edge_Accent_Trimless-LED50_GEN2_Plus-36Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-813Lumen-36Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-36-90-500mA.ies,2700,1,1,0
LED50-GEN2-Plus-22Degrees-2700K-90-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50/2-27-22-90,Pinhole_Edge_Accent_Trimless-LED50_GEN2_Plus-22Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-867Lumen-22Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-22-90-500mA.ies,2700,1,1,0
LED50-Warm-Dim-36Degrees-3000K-80-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 Ambiance WarmDim Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED50WD-30-36,Pinhole_Edge_Accent_Trimless-LED50_Warm_Dim-36Degrees-3000K-80-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,96 x 92 x 92,14.5,14.5,Xtech_Lucent_Pinhole_Edge-LED50_Warm_Dim-568Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED - LED50WD-30-36-700mA.ies,3000,2,1,0
LED50-One-GEN2-24Degrees-3000K-90-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 ONE GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED51/2-30-24,Pinhole_Edge_Accent_Trimless-LED50_One_GEN2-24Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-LED50_One_GEN2-1082Lumen-24Degrees-3000K-90-CRI,91413-A_F-LED - LED51_2-30-24-350mA.ies,3000,2,1,0
LED50-One-Superspot-7Degrees-3000K-90-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with LED50 ONE SuperSpot Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-LED-BK-PC-LED51-30-7,Pinhole_Edge_Accent_Trimless-LED50_One_Superspot-7Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/94166/91413-a-led.pdf,90 x 92 x 92,6.7,6.7,Xtech_Lucent_Pinhole_Edge-LED50_One_Superspot-486Lumen-7Degrees-3000K-90-CRI,91413-A_F-LED - LED51SS-30-7-350mA.ies,3000,2,1,0
XTM-1300Lumen-55Degrees-3000K-83-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with Xicato XTM Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XTM-1300-30-55-5,Pinhole_Edge_Accent_Trimless-XTM-55Degrees-3000K-83-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,132 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-XTM-1300Lumen-55Degrees-3000K-83-CRI,91413-XIC-XTM-0D-1300-xx-55-5-700.ies,3000,5,1,0
XTA-1300Lumen-55Degrees-2700K-98-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with Xicato XTA Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XTA-1300-27-55-5,Pinhole_Edge_Accent_Trimless-XTA-55Degrees-2700K-98-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,132 x 92 x 92,15.6,15.6,Xtech_Lucent_Pinhole_Edge-XTA-1300Lumen-55Degrees-2700K-98-CRI,91413-XIC-XTA-0D-1300-xx-55-5-700.ies,2700,5,1,0
XTM9-1300Lumen-37Degrees-3000K-83-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with Xicato XTM9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XTM9-1300-30-37-5,Pinhole_Edge_Accent_Trimless-XTM9-37Degrees-3000K-83-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,118 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XTM9-1300Lumen-37Degrees-3000K-83-CRI,91413-F_A-XIC - XTM09-0D-1300-xx-15-5-700mA.ies,3000,4,1,0
XTA9-37Degrees-3000K-98-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with Xicato XTA9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XTA9-700-30-37-5,Pinhole_Edge_Accent_Trimless-XTA9-37Degrees-3000K-98-CRI-Lucent,85,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,85 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XTA9-37Degrees-3000K-98-CRI,91413-F_A-XIC - XTA09-0D-1300-xx-15-5-1050mA.ies,3000,3,1,0
XLED50-Shallow-Height-23Degrees-2700K-83-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XLED50-827-23-SH,Pinhole_Edge_Accent_Trimless-XLED50_Shallow_Height-23Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-23Degrees-2700K-83-CRI,,2700,6,1,0
XLED50-Shallow-Height-35Degrees-2700K-83-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XLED50-827-35-SH,Pinhole_Edge_Accent_Trimless-XLED50_Shallow_Height-35Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-35Degrees-2700K-83-CRI,,2700,6,1,0
XLED50-High-Efficency-35Degrees-3000K-83-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XLED50-830-35-HE,Pinhole_Edge_Accent_Trimless-XLED50_High_Efficency-35Degrees-3000K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-35Degrees-3000K-83-CRI,,3000,7,1,0
XLED50-High-Efficency-23Degrees-2700K-83-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XLED50-827-23-HE,Pinhole_Edge_Accent_Trimless-XLED50_High_Efficency-23Degrees-2700K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-23Degrees-2700K-83-CRI,,2700,7,1,0
XLED50-High-Output-23Degrees-2700K-83-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with XLED50 High Output Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XLED50-HO-927-23,Pinhole_Edge_Accent_Trimless-XLED50_High_Output-23Degrees-2700K-83-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_Output-23Degrees-2700K-83-CRI,,2700,8,1,0
XLED50-Shallow-Height-High-CRI-23Degrees-3000K-98-CRI-Adjustable-Trimless-Black,RAL 9005,"Adjustable Pinhole Edge Trimless with XLED50 Shallow Height, High CRI Module","Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XLED50-SH-90-930-23,Pinhole_Edge_Accent_Trimless-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,96 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI,,3000,7,1,0
XLED50-High-CRI-23Degrees-3000K-98-CRI-Adjustable-Trimless-Black,RAL 9005,Adjustable Pinhole Edge Trimless with XLED50 High CRI Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent/,91413-A-XIC-BK-PC-XLED50-90-930-23,Pinhole_Edge_Accent_Trimless-XLED50_High_CRI-23Degrees-3000K-98-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107606/91413-a-xic.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_CRI-23Degrees-3000K-98-CRI,,3000,8,1,0
LED50-GEN2-22Degrees-2700K-80-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-27-22,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-22Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-624Lumen-22Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-22-500mA.ies,2700,1,0,1
LED50-GEN2-36Degrees-2700K-80-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-27-36,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-36Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-576Lumen-36Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-36-500mA.ies,2700,1,0,1
LED50-GEN2-36Degrees-3000K-80-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-30-36,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-36Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-658Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-36-500mA.ies,3000,1,0,1
LED50-GEN2-18Degrees-3000K-80-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-30-18,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-18Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-683Lumen-18Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-18-500mA.ies,3000,1,0,1
LED50-GEN2-22Degrees-3000K-80-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-30-22,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2-22Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-715Lumen-22Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-22-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-18Degrees-3000K-90-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-30-18-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-18Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-869Lumen-18Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-18-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-36Degrees-3000K-90-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-30-36-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-36Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-823Lumen-36Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-36-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-22Degrees-3000K-90-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-30-22-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-22Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-883Lumen-22Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-22-90-500mA.ies,3000,1,0,1
LED50-GEN2-Plus-36Degrees-2700K-90-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-27-36-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-36Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-813Lumen-36Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-36-90-500mA.ies,2700,1,0,1
LED50-GEN2-Plus-22Degrees-2700K-90-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50/2-27-22-90,Pinhole_Edge_Accent_Trim_IP54-LED50_GEN2_Plus-22Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-867Lumen-22Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-22-90-500mA.ies,2700,1,0,1
LED50-Warm-Dim-36Degrees-3000K-80-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 Ambiance WarmDim Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED50WD-30-36,Pinhole_Edge_Accent_Trim_IP54-LED50_Warm_Dim-36Degrees-3000K-80-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,96 x 92 x 92,14.5,14.5,Xtech_Lucent_Pinhole_Edge-LED50_Warm_Dim-568Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED - LED50WD-30-36-700mA.ies,3000,2,0,1
LED50-One-GEN2-24Degrees-3000K-90-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 ONE GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED51/2-30-24,Pinhole_Edge_Accent_Trim_IP54-LED50_One_GEN2-24Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-LED50_One_GEN2-1082Lumen-24Degrees-3000K-90-CRI,91413-A_F-LED - LED51_2-30-24-350mA.ies,3000,2,0,1
LED50-One-Superspot-7Degrees-3000K-90-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with LED50 ONE SuperSpot Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PB-LED51-30-7,Pinhole_Edge_Accent_Trim_IP54-LED50_One_Superspot-7Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,6.7,6.7,Xtech_Lucent_Pinhole_Edge-LED50_One_Superspot-486Lumen-7Degrees-3000K-90-CRI,91413-A_F-LED - LED51SS-30-7-350mA.ies,3000,2,0,1
XTM-1300Lumen-55Degrees-3000K-83-CRI-Adjustable-IP54-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with Xicato XTM Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XTM-1300-30-55-5,Pinhole_Edge_Accent_Trim_IP54-XTM-55Degrees-3000K-83-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-XTM-1300Lumen-55Degrees-3000K-83-CRI,91413-XIC-XTM-0D-1300-xx-55-5-700.ies,3000,5,0,1
XTA-1300Lumen-55Degrees-2700K-98-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with Xicato XTA Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XTA-1300-27-55-5,Pinhole_Edge_Accent_Trim_IP54-XTA-55Degrees-2700K-98-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,15.6,15.6,Xtech_Lucent_Pinhole_Edge-XTA-1300Lumen-55Degrees-2700K-98-CRI,91413-XIC-XTA-0D-1300-xx-55-5-700.ies,2700,5,0,1
XTM9-1300Lumen-37Degrees-3000K-83-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with Xicato XTM9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XTM9-1300-30-37-5,Pinhole_Edge_Accent_Trim_IP54-XTM9-37Degrees-3000K-83-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,118 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XTM9-1300Lumen-37Degrees-3000K-83-CRI,91413-F_A-XIC - XTM09-0D-1300-xx-15-5-700mA.ies,3000,4,0,1
XTA9-37Degrees-3000K-98-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with Xicato XTA9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XTA9-700-30-37-5,Pinhole_Edge_Accent_Trim_IP54-XTA9-37Degrees-3000K-98-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,118 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XTA9-37Degrees-3000K-98-CRI,91413-F_A-XIC - XTA09-0D-1300-xx-15-5-1050mA.ies,3000,3,0,1
XLED50-Shallow-Height-23Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XLED50-827-23-SH,Pinhole_Edge_Accent_Trim_IP54-XLED50_Shallow_Height-23Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-23Degrees-2700K-83-CRI,,2700,6,0,1
XLED50-Shallow-Height-35Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XLED50-827-35-SH,Pinhole_Edge_Accent_Trim_IP54-XLED50_Shallow_Height-35Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-35Degrees-2700K-83-CRI,,2700,6,0,1
XLED50-High-Efficency-35Degrees-3000K-83-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XLED50-830-35-HE,Pinhole_Edge_Accent_Trim_IP54-XLED50_High_Efficency-35Degrees-3000K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-35Degrees-3000K-83-CRI,,3000,7,0,1
XLED50-High-Efficency-23Degrees-2700K-83-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XLED50-827-23-HE,Pinhole_Edge_Accent_Trim_IP54-XLED50_High_Efficency-23Degrees-2700K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-23Degrees-2700K-83-CRI,,2700,7,0,1
XLED50-High-Output-23Degrees-2700K-83-CRI-Adjustable-IP54-Trim-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trim with XLED50 High Output Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XLED50-HO-927-23,Pinhole_Edge_Accent_Trim_IP54-XLED50_High_Output-23Degrees-2700K-83-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_Output-23Degrees-2700K-83-CRI,,2700,8,0,1
XLED50-Shallow-Height-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Shallow Height-Trim-Black,RAL 9005,"Adjustable IP54 Pinhole Edge Trim with XLED50 Shallow Height, High CRI Module","Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PB-XLED50-SH-90-930-23,Pinhole_Edge_Accent_Trim_IP54-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI,,3000,7,0,1
LED50-GEN2-22Degrees-2700K-80-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-27-22,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-22Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-624Lumen-22Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-22-500mA.ies,2700,1,1,0
LED50-GEN2-36Degrees-2700K-80-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-27-36,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-36Degrees-2700K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-576Lumen-36Degrees-2700K-80-CRI,91413-F_A-LED -LED50_2-27-36-500mA.ies,2700,1,1,0
LED50-GEN2-36Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-30-36,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-36Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-658Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-36-500mA.ies,3000,1,1,0
LED50-GEN2-18Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-30-18,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-18Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-683Lumen-18Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-18-500mA.ies,3000,1,1,0
LED50-GEN2-22Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-30-22,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2-22Degrees-3000K-80-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2-715Lumen-22Degrees-3000K-80-CRI,91413-F_A-LED -LED50_2-30-22-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-18Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-30-18-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-18Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-869Lumen-18Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-18-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-36Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-30-36-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-36Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-823Lumen-36Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-36-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-22Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-30-22-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-22Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-883Lumen-22Degrees-3000K-90-CRI,91413-A_F-LED-LED50_2-30-22-90-500mA.ies,3000,1,1,0
LED50-GEN2-Plus-36Degrees-2700K-90-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-27-36-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-36Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-813Lumen-36Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-36-90-500mA.ies,2700,1,1,0
LED50-GEN2-Plus-22Degrees-2700K-90-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 Plus GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50/2-27-22-90,Pinhole_Edge_Accent_Trimless_IP54-LED50_GEN2_Plus-22Degrees-2700K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,14,14,Xtech_Lucent_Pinhole_Edge-LED50_GEN2_Plus-867Lumen-22Degrees-2700K-90-CRI,91413-A_F-LED-LED50_2-27-22-90-500mA.ies,2700,1,1,0
LED50-Warm-Dim-36Degrees-3000K-80-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 Ambiance WarmDim Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED50WD-30-36,Pinhole_Edge_Accent_Trimless_IP54-LED50_Warm_Dim-36Degrees-3000K-80-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,96 x 92 x 92,14.5,14.5,Xtech_Lucent_Pinhole_Edge-LED50_Warm_Dim-568Lumen-36Degrees-3000K-80-CRI,91413-F_A-LED - LED50WD-30-36-700mA.ies,3000,2,1,0
LED50-One-GEN2-24Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 ONE GEN2 Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED51/2-30-24,Pinhole_Edge_Accent_Trimless_IP54-LED50_One_GEN2-24Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-LED50_One_GEN2-1082Lumen-24Degrees-3000K-90-CRI,91413-A_F-LED - LED51_2-30-24-350mA.ies,3000,2,1,0
LED50-One-Superspot-7Degrees-3000K-90-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with LED50 ONE SuperSpot Module,Adjustable,Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-LED-54-BK-PC-LED51-30-7,Pinhole_Edge_Accent_Trimless_IP54-LED50_One_Superspot-7Degrees-3000K-90-CRI-Lucent,90,92,92,http://www.lucent-lighting.com/media/95257/91413-a-led-54.pdf,90 x 92 x 92,6.7,6.7,Xtech_Lucent_Pinhole_Edge-LED50_One_Superspot-486Lumen-7Degrees-3000K-90-CRI,91413-A_F-LED - LED51SS-30-7-350mA.ies,3000,2,1,0
XTM-1300Lumen-55Degrees-3000K-83-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with Xicato XTM Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XTM-1300-30-55-5,Pinhole_Edge_Accent_Trimless_IP54-XTM-55Degrees-3000K-83-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,13.8,13.8,Xtech_Lucent_Pinhole_Edge-XTM-1300Lumen-55Degrees-3000K-83-CRI,91413-XIC-XTM-0D-1300-xx-55-5-700.ies,3000,5,1,0
XTA-1300Lumen-55Degrees-2700K-98-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with Xicato XTA Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XTA-1300-27-55-5,Pinhole_Edge_Accent_Trimless_IP54-XTA-55Degrees-2700K-98-CRI-Lucent,132,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,132 x 92 x 92,15.6,15.6,Xtech_Lucent_Pinhole_Edge-XTA-1300Lumen-55Degrees-2700K-98-CRI,91413-XIC-XTA-0D-1300-xx-55-5-700.ies,2700,5,1,0
XTM9-1300Lumen-37Degrees-3000K-83-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with Xicato XTM9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XTM9-1300-30-37-5,Pinhole_Edge_Accent_Trimless_IP54-XTM9-37Degrees-3000K-83-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,118 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XTM9-1300Lumen-37Degrees-3000K-83-CRI,91413-F_A-XIC - XTM09-0D-1300-xx-15-5-700mA.ies,3000,4,1,0
XTA9-37Degrees-3000K-98-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with Xicato XTA9 Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XTA9-700-30-37-5,Pinhole_Edge_Accent_Trimless_IP54-XTA9-37Degrees-3000K-98-CRI-Lucent,118,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,118 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XTA9-37Degrees-3000K-98-CRI,91413-F_A-XIC - XTA09-0D-1300-xx-15-5-1050mA.ies,3000,3,1,0
XLED50-Shallow-Height-23Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XLED50-827-23-SH,Pinhole_Edge_Accent_Trimless_IP54-XLED50_Shallow_Height-23Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-23Degrees-2700K-83-CRI,,2700,6,1,0
XLED50-Shallow-Height-35Degrees-2700K-83-CRI-Adjustable-IP54-Shallow Height-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with XLED50 Shallow Height Module,"Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XLED50-827-35-SH,Pinhole_Edge_Accent_Trimless_IP54-XLED50_Shallow_Height-35Degrees-2700K-83-CRI-Lucent,78,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,78 x 92 x 92,9.2,9.2,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height-35Degrees-2700K-83-CRI,,2700,6,1,0
XLED50-High-Efficency-35Degrees-3000K-83-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XLED50-830-35-HE,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_Efficency-35Degrees-3000K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-35Degrees-3000K-83-CRI,,3000,7,1,0
XLED50-High-Efficency-23Degrees-2700K-83-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with XLED50 High Efficiency Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XLED50-827-23-HE,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_Efficency-23Degrees-2700K-83-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,12.8,12.8,Xtech_Lucent_Pinhole_Edge-XLED50_High_Efficency-23Degrees-2700K-83-CRI,,2700,7,1,0
XLED50-High-Output-23Degrees-2700K-83-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with XLED50 High Output Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XLED50-HO-927-23,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_Output-23Degrees-2700K-83-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_Output-23Degrees-2700K-83-CRI,,2700,8,1,0
XLED50-Shallow-Height-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Shallow Height-Trimless-Black,RAL 9005,"Adjustable IP54 Pinhole Edge Trimless with XLED50 Shallow Height, High CRI Module","Adjustable, IP54, Shallow Height",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XLED50-SH-90-930-23,Pinhole_Edge_Accent_Trimless_IP54-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI-Lucent,96,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,96 x 92 x 92,11.4,11.4,Xtech_Lucent_Pinhole_Edge-XLED50_Shallow_Height_High_CRI-23Degrees-3000K-98-CRI,,3000,7,1,0
XLED50-High-CRI-23Degrees-3000K-98-CRI-Adjustable-IP54-Trimless-Black,RAL 9005,Adjustable IP54 Pinhole Edge Trimless with XLED50 High CRI Module,"Adjustable, IP54",Powder Coat - Lucent - Black RAL 9005,Xtech_Lucent_Black_RAL9005,http://www.lucent-lighting.com/products/prospex-light-fixtures/pinhole-downlights/pinhole-edge/pinhole-edge-90-accent-ip54/,91413-A-XIC-54-BK-PC-XLED50-90-930-23,Pinhole_Edge_Accent_Trimless_IP54-XLED50_High_CRI-23Degrees-3000K-98-CRI-Lucent,111,92,92,http://www.lucent-lighting.com/media/107604/91413-a-xic-54.pdf,111 x 92 x 92,18.4,18.4,Xtech_Lucent_Pinhole_Edge-XLED50_High_CRI-23Degrees-3000K-98-CRI,,3000,8,1,0
